**9. LIMITATION AND FUTURE ENHANCEMENT**

**LIMITATION**

* Area is limited for server and display as Zig-Bee can cover 50-70mtrs only.
* We have used 16x2 LCD Display so we cannot display large message in once, for displaying it fragmentation should be done.
* Though Zig-Bee consumes very law battery cost of each module is very high as compared to Bluetooth module.

**FUTURE ENHANCEMENT**

* A Graphics LCD can be attached to the system to display large data in once and it will increase readability of the display too.
* Though Bluetooth has very low coverage area yet we can use combination of Bluetooth and Zig-Bee to increase the Coverage area of the system and to add more nodes connected to the server cost effectively.
* It can be connected to any other device likewise:-RFID reader to display info about lecture automatically, strength in the class, Automatic change when lecture changes.

.